***************************************************************************
* MOBILE6.2 (31-Oct-2002)                                                 *
* Input file: 93.IN (file 1, run 1).                                      *
***************************************************************************
* Longmont Colorado Compliance Rates
*MAXIMUM I/M BENEFIT
* Basic I/M Program -- Idle Testing for pre-1982 GAS VEHICLES
* Default Cutpoints
  M616 Comment:
               User has supplied post-1999 sulfur levels.

* Reading Registration Distributions from the following external
* data file: ../../REGDIST/REG_MET.D
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   urb  1993da                                                                                                      
* File 1, Run 1, Scenario 1.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

          User supplied gasoline sulfur content = 186.0 ppm.


* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\URB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\URB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\URB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
*** I/M credits for Tech1&2 vehicles were read from the following external
    data file: TECH12.D                                                                        
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  1993
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.9 psi
                    Weathered RVP:  13.2 psi
              Fuel Sulfur Content:  186. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.550       Alcohol Blend Market Share: 0.450
   Ether Blend Oxygen Content: 0.027     Alcohol Blend Oxygen Content: 0.035
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.7038    0.1648    0.0838              0.0126    0.0079    0.0023    0.0247    0.0000    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      3.69      3.23      6.59      4.37      5.77      1.15      2.15      3.68      0.00     3.863
     Composite CO  :     52.05     46.97     72.11     55.44    104.71      2.47      4.36     21.52      0.00    52.300
     Composite NOX :      2.73      2.15      2.47      2.26      5.00      1.70      2.03     18.31      0.00     3.017
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   sub  1993da                                                                                                      
* File 1, Run 1, Scenario 2.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

          User supplied gasoline sulfur content = 186.0 ppm.


* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\SUB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\SUB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\SUB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  1993
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.9 psi
                    Weathered RVP:  13.2 psi
              Fuel Sulfur Content:  186. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.550       Alcohol Blend Market Share: 0.450
   Ether Blend Oxygen Content: 0.027     Alcohol Blend Oxygen Content: 0.035
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.6575    0.1882    0.0958              0.0164    0.0074    0.0026    0.0320    0.0000    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      3.56      3.13      6.41      4.23      4.75      1.05      1.98      3.19      0.00     3.738
     Composite CO  :     52.32     47.44     72.19     55.78     90.33      2.26      4.02     18.40      0.00    52.345
     Composite NOX :      2.72      2.15      2.46      2.26      5.24      1.68      2.01     18.28      0.00     3.121
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   rur  1993da                                                                                                      
* File 1, Run 1, Scenario 3.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

          User supplied gasoline sulfur content = 186.0 ppm.


* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\RUR.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\RUR.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\RUR.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  1993
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.9 psi
                    Weathered RVP:  13.2 psi
              Fuel Sulfur Content:  186. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.550       Alcohol Blend Market Share: 0.450
   Ether Blend Oxygen Content: 0.027     Alcohol Blend Oxygen Content: 0.035
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.5768    0.2170    0.1107              0.0290    0.0065    0.0030    0.0569    0.0000    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      3.36      2.96      6.12      4.03      3.20      0.90      1.73      2.44      0.00     3.500
     Composite CO  :     53.29     48.80     72.97     56.97     70.44      1.95      3.52     13.85      0.00    52.265
     Composite NOX :      2.75      2.19      2.50      2.30      5.63      1.72      2.06     19.22      0.00     3.615
  ----------------------------------------------------------------------------------------------------------------------
