***************************************************************************
* MOBILE6.2 (31-Oct-2002)                                                 *
* Input file: 10.IN (file 1, run 1).                                      *
***************************************************************************
* Evaluation year 2010 only
* Program data from inspection year 2001
* Basic and Enhanced I/M Programs
* Pass/fail Idle/2500 for all HDGV vehicles >1981
* Colorado 2010 I/M240 cutpoints for cars and trucks

* Reading non-default I/M CUTPOINTS from the following external
* data file: 10CUTPC.D                                                                       

* Reading non-default I/M CUTPOINTS from the following external
* data file: 10CUTPT.D                                                                       
  M616 Comment:
               User has supplied post-1999 sulfur levels.
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   urb  2010QA                                                                                                      
* File 1, Run 1, Scenario 1.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\URB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\URB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\URB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
*** I/M credits for Tech1&2 vehicles were read from the following external
    data file: TECH12.D                                                                        
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2010
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.015
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3735    0.4122    0.1406              0.0195    0.0003    0.0021    0.0495    0.0024    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.582     0.796     1.464     0.966     1.274    0.197     0.502     0.913      2.54     0.828
     Composite CO  :     17.63     20.66     25.80     21.97     32.07     1.118     0.984     4.957     27.25    19.664
     Composite NOX :      0.588     0.891     1.426     1.027     2.004    0.382     0.676     6.784      1.09     1.166
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   sub  2010QA                                                                                                      
* File 1, Run 1, Scenario 2.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\SUB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\SUB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\SUB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2010
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.015
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3229    0.4510    0.1539              0.0190    0.0003    0.0023    0.0482    0.0025    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.562     0.774     1.418     0.938     1.111    0.181     0.460     0.798      2.40     0.815
     Composite CO  :     17.91     20.98     26.15     22.29     28.32     1.028     0.908     4.314     25.12    20.078
     Composite NOX :      0.587     0.887     1.418     1.022     2.091    0.381     0.675     6.697      1.16     1.175
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   rur  2010QA                                                                                                      
* File 1, Run 1, Scenario 3.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\RUR.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\RUR.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\RUR.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2010
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.015
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3318    0.4400    0.1500              0.0204    0.0003    0.0022    0.0502    0.0051    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.530     0.740     1.346     0.894     0.844    0.156     0.397     0.624      2.19     0.764
     Composite CO  :     18.57     21.70     26.99     23.05     22.44     0.889     0.792     3.315     22.33    20.501
     Composite NOX :      0.599     0.901     1.434     1.037     2.209    0.387     0.686     6.812      1.26     1.205
  ----------------------------------------------------------------------------------------------------------------------
