***************************************************************************
* MOBILE6.2 (31-Oct-2002)                                                 *
* Input file: 05.IN (file 1, run 1).                                      *
***************************************************************************
* Evaluation year 2005 only
* Program data from inspection year 2000
* Basic and Enhanced I/M Programs
* Pass/fail Idle only for all HDGV vehicles >1981
* Colorado 2005 I/M240 cutpoints for cars and trucks

* Reading non-default I/M CUTPOINTS from the following external
* data file: 05CUTPC.D                                                                       

* Reading non-default I/M CUTPOINTS from the following external
* data file: 05CUTPT.D                                                                       
  M616 Comment:
               User has supplied post-1999 sulfur levels.

* Reading Registration Distributions from the following external
* data file: ../../REGDIST/REG_MET.D
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   urb  2001FA                                                                                                      
* File 1, Run 1, Scenario 1.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\URB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\URB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\URB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
*** I/M credits for Tech1&2 vehicles were read from the following external
    data file: TECH12.D                                                                        
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2005
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.019
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4418    0.3615    0.1234              0.0194    0.0013    0.0019    0.0480    0.0027    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.306     1.222     2.933     1.657     2.239    1.205     0.877     1.249      6.69     1.505
     Composite CO  :     27.52     28.27     30.92     28.95     42.25     2.796     2.179     7.412     36.16    27.473
     Composite NOX :      1.212     1.340     1.661     1.422     3.774    1.616     1.152    10.482      1.35     1.809
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   sub  2001FA                                                                                                      
* File 1, Run 1, Scenario 2.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\SUB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\SUB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\SUB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2005
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.019
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3915    0.4003    0.1366              0.0189    0.0011    0.0022    0.0467    0.0028    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.251     1.174     2.829     1.595     1.862    1.103     0.799     1.053      6.41     1.451
     Composite CO  :     28.43     29.28     31.76     29.91     36.80     2.605     2.034     6.317     33.70    28.279
     Composite NOX :      1.223     1.353     1.669     1.433     4.014    1.669     1.190    10.955      1.44     1.844
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   rur  2001FA                                                                                                      
* File 1, Run 1, Scenario 3.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\RUR.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\RUR.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\RUR.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2005
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.019
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4003    0.3893    0.1328              0.0203    0.0012    0.0021    0.0486    0.0054    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.194     1.123     2.721     1.529     1.437    1.001     0.721     0.854      6.13     1.383
     Composite CO  :     29.41     30.35     32.63     30.93     30.20     2.401     1.880     5.129     31.32    28.960
     Composite NOX :      1.245     1.378     1.693     1.458     4.208    1.715     1.224    11.461      1.53     1.915
  ----------------------------------------------------------------------------------------------------------------------
