***************************************************************************
* MOBILE6.2 (31-Oct-2002)                                                 *
* Input file: MOBILE6.IN (file 1, run 1).                                 *
***************************************************************************
* Evaluation year 2006 only
* Program data from inspection year 2001
* Basic and Enhanced I/M Programs
* Pass/fail Idle/2500 for all HDGV vehicles >1981
* Colorado 2006 I/M240 cutpoints for cars and trucks
  M616 Comment:
               User has supplied post-1999 sulfur levels.

* Reading Registration Distributions from the following external
* data file: ../../REGDIST/REG_MET.D
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   rur  2006FA                                                                                                      
* File 1, Run 1, Scenario 1.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPDRUR.DEF                                                                      

* Reading Hourly VMT distribution from the following external
* data file: VMTRUR.DEF                                                                      

* Reading Hourly Roadway VMT distribution from the following external
* data file: FVMTRUR.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2006
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.015
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4284    0.3715    0.1266              0.0193    0.0010    0.0023    0.0484    0.0026    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.269     1.136     2.855     1.573     1.352    0.741     0.821     0.777      5.85     1.409
     Composite CO  :     33.38     32.10     36.32     33.17     33.67     2.208     2.263     4.734     31.88    31.791
     Composite NOX :      1.241     1.349     1.652     1.426     3.872    1.587     1.233    10.561      1.55     1.836
  ----------------------------------------------------------------------------------------------------------------------
