***************************************************************************
* MOBILE6.2 (31-Oct-2002)                                                 *
* Input file: 15.IN (file 1, run 1).                                      *
***************************************************************************
* Basic I/M Program
* Idle testing for all HDGV vehicles >1981
* Default Cutpoints
* IM240 Exhaust I/M program for POST-81 MY LDVs
* Colorado cutpoints

* Reading non-default I/M CUTPOINTS from the following external
* data file: 15_CUTP.D                                                                       
  M616 Comment:
               User has supplied post-1999 sulfur levels.
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   urb  20157A                                                                                                      
* File 1, Run 1, Scenario 1.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\URB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\URB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\URB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
*** I/M credits for Tech1&2 vehicles were read from the following external
    data file: TECH12.D                                                                        
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2015
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.9 psi
                    Weathered RVP:  13.5 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3266    0.4469    0.1524              0.0194    0.0003    0.0022    0.0500    0.0022    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.350     0.494     0.965     0.614     0.782    0.105     0.332     0.668      2.50     0.537
     Composite CO  :     15.68     16.93     21.40     18.06     28.00     0.899     0.746     2.234     26.23    16.660
     Composite NOX :      0.326     0.547     1.079     0.682     1.001    0.142     0.395     3.367      1.11     0.707
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   sub  20157A                                                                                                      
* File 1, Run 1, Scenario 2.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\SUB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\SUB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\SUB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2015
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.9 psi
                    Weathered RVP:  13.5 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.2761    0.4857    0.1657              0.0190    0.0002    0.0024    0.0486    0.0023    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.339     0.481     0.933     0.596     0.680    0.095     0.302     0.574      2.37     0.529
     Composite CO  :     16.14     17.45     22.03     18.61     25.28     0.830     0.691     1.947     24.40    17.212
     Composite NOX :      0.331     0.552     1.083     0.687     1.062    0.149     0.415     3.506      1.20     0.733
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   rur  20157A                                                                                                      
* File 1, Run 1, Scenario 3.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\RUR.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\RUR.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\RUR.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2015
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.9 psi
                    Weathered RVP:  13.5 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.2850    0.4747    0.1618              0.0204    0.0003    0.0024    0.0505    0.0049    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.322     0.463     0.890     0.572     0.541    0.083     0.267     0.459      2.19     0.501
     Composite CO  :     16.60     17.94     22.65     19.14     21.12     0.736     0.616     1.540     22.13    17.531
     Composite NOX :      0.337     0.559     1.094     0.695     1.116    0.154     0.430     3.557      1.30     0.748
  ----------------------------------------------------------------------------------------------------------------------
