***************************************************************************
* MOBILE6.2 (31-Oct-2002)                                                 *
* Input file: 05NC.IN (file 1, run 1).                                    *
***************************************************************************
  M616 Comment:
               User has supplied post-1999 sulfur levels.

* Reading Registration Distributions from the following external
* data file: ../../REGDIST/REG_MET.D
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   urb  2001FA                                                                                                      
* File 1, Run 1, Scenario 1.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\URB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\URB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\URB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2005
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.9 psi
                    Weathered RVP:  12.9 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4418    0.3615    0.1234              0.0194    0.0013    0.0019    0.0480    0.0027    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.590     1.434     3.408     1.936     2.428    1.205     0.877     1.249      6.72     1.770
     Composite CO  :     32.88     31.92     38.42     33.57     53.74     2.796     2.179     7.412     41.35    32.323
     Composite NOX :      1.267     1.394     1.708     1.474     3.804    1.616     1.152    10.482      1.35     1.859
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   sub  2001FA                                                                                                      
* File 1, Run 1, Scenario 2.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\SUB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\SUB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\SUB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2005
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.9 psi
                    Weathered RVP:  12.9 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3915    0.4003    0.1366              0.0189    0.0011    0.0022    0.0467    0.0028    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.517     1.372     3.289     1.860     2.007    1.103     0.799     1.053      6.44     1.700
     Composite CO  :     33.86     32.96     39.05     34.51     46.81     2.605     2.034     6.317     38.53    33.076
     Composite NOX :      1.278     1.406     1.716     1.485     4.045    1.669     1.190    10.955      1.44     1.894
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   rur  2001FA                                                                                                      
* File 1, Run 1, Scenario 3.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\RUR.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\RUR.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\RUR.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2005
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  18.0 (F)
              Maximum Temperature:  28.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.9 psi
                    Weathered RVP:  12.9 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4003    0.3893    0.1328              0.0203    0.0012    0.0021    0.0486    0.0054    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.440     1.308     3.165     1.781     1.534    1.001     0.721     0.854      6.16     1.615
     Composite CO  :     34.87     34.05     39.74     35.49     38.39     2.401     1.880     5.129     35.82    33.721
     Composite NOX :      1.300     1.431     1.739     1.510     4.241    1.715     1.224    11.461      1.53     1.965
  ----------------------------------------------------------------------------------------------------------------------
