***************************************************************************
* MOBILE6 (16-Jan-2002)                                                   *
* Input file: 04NC.IN (file 1, run 1).                                    *
***************************************************************************
  M616 Comment:
               User has supplied post-1999 sulfur levels.

* Reading Registration Distributions from the following external
* data file: ../../REGDIST/REG_MET.D
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   cbd  2004FA                                                                                                      
* File 1, Run 1, Scenario 1.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPD_CBD.DEF                                                                     

* Reading Hourly VMT distribution from the following external
* data file: VMT_CBD.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FVMT_CBD.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2004
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  12.5 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No  

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.5125    0.3070    0.1049              0.0142    0.0012    0.0016    0.0542    0.0045    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      2.248     1.706     5.169     2.588     5.520    1.209     1.198     1.811      8.02     2.434
     Composite CO  :     28.14     28.10     55.59     35.10    109.79     2.856     2.229    10.260     40.14    31.187
     Composite NOX :      1.289     1.399     1.926     1.533     4.179    1.739     1.372    13.349      1.11     2.084
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   frn  2004FA                                                                                                      
* File 1, Run 1, Scenario 2.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPD_FRN.DEF                                                                     

* Reading Hourly VMT distribution from the following external
* data file: VMT_FRN.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FVMT_FRN.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2004
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  12.5 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No  

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4712    0.3459    0.1182              0.0168    0.0011    0.0018    0.0425    0.0025    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      2.005     1.520     4.857     2.370     2.474    1.013     1.003     1.163      7.41     2.157
     Composite CO  :     28.63     28.64     55.71     35.53     49.70     2.426     1.888     6.822     34.94    31.201
     Composite NOX :      1.240     1.346     1.857     1.476     3.926    1.763     1.391    13.325      1.28     1.909
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   urb  2004FA                                                                                                      
* File 1, Run 1, Scenario 3.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPD_URB.DEF                                                                     

* Reading Hourly VMT distribution from the following external
* data file: VMT_URB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FVMT_URB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2004
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  12.5 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No  

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4553    0.3518    0.1203              0.0194    0.0010    0.0018    0.0476    0.0028    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      2.010     1.521     4.860     2.372     2.425    1.015     1.005     1.155      7.44     2.160
     Composite CO  :     28.40     28.40     55.49     35.30     48.56     2.434     1.894     6.829     35.52    30.969
     Composite NOX :      1.231     1.335     1.845     1.465     3.882    1.765     1.393    12.908      1.28     1.950
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   sub  2004FA                                                                                                      
* File 1, Run 1, Scenario 4.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPD_SUB.DEF                                                                     

* Reading Hourly VMT distribution from the following external
* data file: VMT_SUB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FVMT_SUB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2004
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  12.5 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No  

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4049    0.3906    0.1336              0.0189    0.0009    0.0020    0.0462    0.0029    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.956     1.481     4.793     2.325     2.210    0.966     0.956     1.046      7.32     2.125
     Composite CO  :     28.99     29.01     56.04     35.90     45.76     2.354     1.831     6.325     34.67    31.815
     Composite NOX :      1.239     1.345     1.853     1.475     4.026    1.833     1.447    13.501      1.33     1.983
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   rur  2004FA                                                                                                      
* File 1, Run 1, Scenario 5.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPD_RUR.DEF                                                                     

* Reading Hourly VMT distribution from the following external
* data file: VMT_RUR.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FVMT_RUR.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2004
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  12.5 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No  

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4138    0.3795    0.1297              0.0202    0.0010    0.0020    0.0483    0.0055    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.867     1.414     4.678     2.246     1.862    0.899     0.890     0.893      7.36     2.040
     Composite CO  :     30.13     30.21     57.10     37.06     43.13     2.269     1.764     5.766     38.71    32.707
     Composite NOX :      1.268     1.378     1.885     1.507     4.230    2.069     1.637    15.411      1.43     2.135
  ----------------------------------------------------------------------------------------------------------------------
