***************************************************************************
* MOBILE6 (16-Jan-2002)                                                   *
* Input file: MOBILE6.IN (file 1, run 1).                                 *
***************************************************************************
* Evaluation year 2005 only
* Program data from inspection year 2000
* Basic and Enhanced I/M Programs
* Pass/fail Idle only for all HDGV vehicles >1981
* Colorado 2005 I/M240 cutpoints for cars and trucks
  M616 Comment:
               User has supplied post-1999 sulfur levels.

* Reading Registration Distributions from the following external
* data file: ../../REGDIST/REG_MET.D
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   rur  2005FA                                                                                                      
* File 1, Run 1, Scenario 1.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPD_RUR.DEF                                                                     

* Reading Hourly VMT distribution from the following external
* data file: VMT_RUR.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FVMT_RUR.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2005
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No  

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.019
                                          Alcohol Blend RVP Waiver: Yes 
       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4003    0.3893    0.1328              0.0203    0.0012    0.0021    0.0486    0.0054    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.452     1.210     2.783     1.610     1.855    1.005     0.723     0.860      7.51     1.545
     Composite CO  :     26.60     26.48     30.87     27.60     36.40     2.500     1.955     5.686     34.86    26.269
     Composite NOX :      1.176     1.290     1.566     1.360     4.137    2.034     1.455    14.289      1.43     1.973
  ----------------------------------------------------------------------------------------------------------------------
