***************************************************************************
* MOBILE6 (16-Jan-2002)                                                   *
* Input file: 05NC.IN (file 1, run 1).                                    *
***************************************************************************
  M616 Comment:
               User has supplied post-1999 sulfur levels.

* Reading Registration Distributions from the following external
* data file: ../../REGDIST/REG_MET.D
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   cbd  2005FA                                                                                                      
* File 1, Run 1, Scenario 1.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPD_CBD.DEF                                                                     

* Reading Hourly VMT distribution from the following external
* data file: VMT_CBD.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FVMT_CBD.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2005
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  12.5 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No  

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.5273    0.2991    0.1022              0.0126    0.0015    0.0016    0.0511    0.0046    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.836     1.502     3.306     1.962     5.195    1.328     0.972     1.720      7.87     1.949
     Composite CO  :     26.00     25.54     33.21     27.49    102.26     3.082     2.396    10.013     40.01    26.733
     Composite NOX :      1.185     1.298     1.589     1.372     4.124    1.677     1.196    12.375      1.11     1.869
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   frn  2005FA                                                                                                      
* File 1, Run 1, Scenario 2.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPD_FRN.DEF                                                                     

* Reading Hourly VMT distribution from the following external
* data file: VMT_FRN.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FVMT_FRN.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2005
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  12.5 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No  

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4846    0.3390    0.1158              0.0154    0.0014    0.0018    0.0393    0.0027    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.605     1.333     3.004     1.759     2.356    1.117     0.809     1.096      7.30     1.680
     Composite CO  :     26.64     26.25     32.99     27.97     47.52     2.637     2.059     6.569     35.42    26.723
     Composite NOX :      1.147     1.255     1.534     1.326     3.884    1.729     1.234    12.305      1.28     1.710
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   urb  2005FA                                                                                                      
* File 1, Run 1, Scenario 3.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPD_URB.DEF                                                                     

* Reading Hourly VMT distribution from the following external
* data file: VMT_URB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FVMT_URB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2005
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  12.5 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No  

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4695    0.3450    0.1177              0.0177    0.0014    0.0019    0.0439    0.0029    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.600     1.328     2.992     1.751     2.260    1.109     0.804     1.069      7.32     1.673
     Composite CO  :     26.50     26.11     32.82     27.82     45.67     2.625     2.050     6.443     36.13    26.519
     Composite NOX :      1.141     1.249     1.526     1.319     3.857    1.739     1.241    12.048      1.29     1.751
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   sub  2005FA                                                                                                      
* File 1, Run 1, Scenario 4.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPD_SUB.DEF                                                                     

* Reading Hourly VMT distribution from the following external
* data file: VMT_SUB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FVMT_SUB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2005
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  12.5 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No  

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4190    0.3842    0.1311              0.0172    0.0012    0.0021    0.0423    0.0030    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.546     1.290     2.923     1.705     2.046    1.054     0.762     0.963      7.19     1.627
     Composite CO  :     27.04     26.67     33.20     28.33     42.59     2.531     1.979     5.905     35.11    27.019
     Composite NOX :      1.149     1.259     1.534     1.329     3.992    1.794     1.281    12.497      1.34     1.773
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   rur  2005FA                                                                                                      
* File 1, Run 1, Scenario 5.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPD_RUR.DEF                                                                     

* Reading Hourly VMT distribution from the following external
* data file: VMT_RUR.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FVMT_RUR.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2005
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  12.5 psi
              Fuel Sulfur Content:  160. ppm

              Exhaust I/M Program:  No  
                 Evap I/M Program:  No  
                      ATP Program:  No  
                 Reformulated Gas:  No  

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4284    0.3730    0.1273              0.0183    0.0012    0.0020    0.0442    0.0055    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.487     1.247     2.844     1.653     1.831    1.005     0.723     0.861      7.30     1.579
     Composite CO  :     28.06     27.71     34.04     29.32     42.49     2.500     1.955     5.690     39.86    27.949
     Composite NOX :      1.174     1.287     1.561     1.357     4.163    2.034     1.455    14.301      1.43     1.903
  ----------------------------------------------------------------------------------------------------------------------
