***************************************************************************
* MOBILE6.2 (31-Oct-2002)                                                 *
* Input file: 13CAL3.IN (file 1, run 1).                                  *
***************************************************************************
* Evaluation year 2013 only
* Program data from inspection year 2001
* Basic and Enhanced I/M Programs
* Pass/fail Idle/2500 for all HDGV vehicles >1981
* Colorado 2013 I/M240 cutpoints for cars and trucks

* Reading non-default I/M CUTPOINTS from the following external
* data file: 13CUTPC.D                                                                       

* Reading non-default I/M CUTPOINTS from the following external
* data file: 13CUTPT.D                                                                       
  M616 Comment:
               User has supplied post-1999 sulfur levels.

* Reading Registration Distributions from the following external
* data file: ../../REGDIST/REG_MET.D
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   AM-running cbd  2013QA                                                                                           
* File 1, Run 1, Scenario 1.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\CBD.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\AMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
*** I/M credits for Tech1&2 vehicles were read from the following external
    data file: TECH12.D                                                                        
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3999    0.3904    0.1331              0.0116    0.0004    0.0020    0.0588    0.0039    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.788     0.625     1.552     0.861     1.825    0.196     0.391     1.271      7.80     0.893
     Composite CO  :     14.46     14.23     19.89     15.67     48.64     1.373     1.004     5.654     40.81    15.044
     Composite NOX :      0.567     0.626     1.040     0.731     1.394    0.293     0.396     6.579      1.09     1.017
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG  AM-running frn  2013QA                                                                                            
* File 1, Run 1, Scenario 2.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\FRN.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\AMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3584    0.4294    0.1464              0.0167    0.0003    0.0022    0.0448    0.0019    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.721     0.573     1.436     0.792     1.226    0.172     0.345     0.887      7.21     0.789
     Composite CO  :     13.84     13.59     19.06     14.98     34.24     1.153     0.848     3.579     36.02    14.390
     Composite NOX :      0.525     0.579     0.973     0.679     1.129    0.269     0.364     4.442      1.16     0.800
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG AM-running  urb  2013QA                                                                                            
* File 1, Run 1, Scenario 3.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\URB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\AMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3426    0.4353    0.1485              0.0193    0.0003    0.0022    0.0497    0.0022    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.682     0.543     1.367     0.753     1.042    0.155     0.312     0.753      6.90     0.746
     Composite CO  :     13.53     13.26     18.63     14.63     27.53     1.010     0.746     2.864     33.40    13.921
     Composite NOX :      0.502     0.554     0.937     0.651     1.152    0.254     0.343     4.065      1.21     0.780
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG AM-running  sub  2013QA                                                                                            
* File 1, Run 1, Scenario 4.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\SUB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\AMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.2920    0.4741    0.1618              0.0189    0.0003    0.0024    0.0483    0.0023    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.659     0.527     1.325     0.730     0.927    0.141     0.286     0.653      6.68     0.722
     Composite CO  :     13.63     13.36     18.74     14.73     23.55     0.915     0.679     2.424     31.12    13.981
     Composite NOX :      0.496     0.547     0.925     0.643     1.199    0.250     0.337     3.967      1.28     0.772
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG AM-idle  cbd  2013QA                                                                                               
* File 1, Run 1, Scenario 5.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\IDLE.DEF                                                                  

* Reading Hourly VMT distribution from the following external
* data file: VMT\AMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3999    0.3904    0.1331              0.0116    0.0004    0.0020    0.0588    0.0039    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      3.708     2.465     5.873     3.331     7.098    0.334     0.656     2.471     17.49     3.524
     Composite CO  :     32.42     31.54     41.82     34.16    138.62     3.014     2.165    14.981    113.24    33.782
     Composite NOX :      0.897     0.999     1.596     1.151     1.199    0.466     0.628    10.628      1.19     1.606
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG  AM-idle  frn  2013QA                                                                                              
* File 1, Run 1, Scenario 6.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\IDLE.DEF                                                                  

* Reading Hourly VMT distribution from the following external
* data file: VMT\AMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3584    0.4294    0.1464              0.0167    0.0003    0.0022    0.0448    0.0019    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      3.708     2.465     5.874     3.332     5.677    0.334     0.656     2.067     17.49     3.469
     Composite CO  :     32.42     31.54     41.82     34.16    127.02     3.014     2.165    12.188    113.24    34.175
     Composite NOX :      0.897     0.999     1.596     1.151     0.928    0.466     0.628     7.763      1.19     1.351
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG  AM-idle  urb  2013QA                                                                                              
* File 1, Run 1, Scenario 7.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\IDLE.DEF                                                                  

* Reading Hourly VMT distribution from the following external
* data file: VMT\AMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3426    0.4353    0.1485              0.0193    0.0003    0.0022    0.0497    0.0022    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      3.708     2.465     5.874     3.332     5.615    0.334     0.656     2.034     17.49     3.465
     Composite CO  :     32.42     31.54     41.82     34.16    126.51     3.014     2.165    11.967    113.24    34.337
     Composite NOX :      0.897     0.999     1.596     1.151     0.916    0.466     0.628     7.530      1.19     1.375
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG  AM-idle  sub  2013QA                                                                                              
* File 1, Run 1, Scenario 8.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\IDLE.DEF                                                                  

* Reading Hourly VMT distribution from the following external
* data file: VMT\AMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.2920    0.4741    0.1618              0.0189    0.0003    0.0024    0.0483    0.0023    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      3.708     2.465     5.875     3.332     5.608    0.334     0.656     2.028     17.49     3.447
     Composite CO  :     32.42     31.54     41.83     34.16    126.49     3.014     2.165    11.913    113.24    34.416
     Composite NOX :      0.897     0.999     1.596     1.151     0.915    0.466     0.628     7.481      1.19     1.377
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   PM-running cbd  2013QA                                                                                           
* File 1, Run 1, Scenario 9.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\CBD.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\PMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3999    0.3904    0.1331              0.0116    0.0004    0.0020    0.0588    0.0039    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.885     0.653     1.624     0.900     1.716    0.184     0.368     1.164      7.43     0.943
     Composite CO  :     13.78     13.48     18.88     14.86     40.71     1.243     0.911     4.910     36.88    14.195
     Composite NOX :      0.498     0.547     0.917     0.641     1.317    0.278     0.376     6.230      1.04     0.921
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG  PM-running frn  2013QA                                                                                            
* File 1, Run 1, Scenario 10.                                                     
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\FRN.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\PMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3584    0.4294    0.1464              0.0167    0.0003    0.0022    0.0448    0.0019    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.783     0.592     1.491     0.820     1.145    0.159     0.321     0.796      6.99     0.822
     Composite CO  :     13.35     13.04     18.31     14.38     28.20     1.038     0.766     3.047     33.17    13.739
     Composite NOX :      0.469     0.514     0.870     0.605     1.072    0.256     0.346     4.213      1.12     0.726
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG PM-running  urb  2013QA                                                                                            
* File 1, Run 1, Scenario 11.                                                     
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\URB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\PMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3426    0.4353    0.1485              0.0193    0.0003    0.0022    0.0497    0.0022    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.747     0.570     1.438     0.791     1.027    0.147     0.298     0.699      6.79     0.788
     Composite CO  :     13.24     12.92     18.15     14.25     24.26     0.948     0.703     2.584     31.31    13.523
     Composite NOX :      0.458     0.501     0.852     0.591     1.089    0.247     0.334     3.950      1.17     0.722
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG PM-running  sub  2013QA                                                                                            
* File 1, Run 1, Scenario 12.                                                     
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\SUB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\PMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.2920    0.4741    0.1618              0.0189    0.0003    0.0024    0.0483    0.0023    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.705     0.547     1.379     0.758     0.900    0.132     0.268     0.585      6.53     0.749
     Composite CO  :     13.41     13.09     18.33     14.42     20.26     0.847     0.631     2.117     28.59    13.639
     Composite NOX :      0.451     0.494     0.840     0.582     1.145    0.245     0.330     3.883      1.24     0.715
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG PM-idle  cbd  2013QA                                                                                               
* File 1, Run 1, Scenario 13.                                                     
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\IDLE.DEF                                                                  

* Reading Hourly VMT distribution from the following external
* data file: VMT\PMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3999    0.3904    0.1331              0.0116    0.0004    0.0020    0.0588    0.0039    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      6.041     3.631     8.913     4.974     9.738    0.334     0.656     2.471     17.53     5.347
     Composite CO  :     31.74     30.71     40.55     33.21    136.58     3.014     2.165    14.981    108.23    32.971
     Composite NOX :      0.823     0.912     1.456     1.050     1.117    0.466     0.628    10.628      1.12     1.522
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG  PM-idle  frn  2013QA                                                                                              
* File 1, Run 1, Scenario 14.                                                     
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\IDLE.DEF                                                                  

* Reading Hourly VMT distribution from the following external
* data file: VMT\PMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3584    0.4294    0.1464              0.0167    0.0003    0.0022    0.0448    0.0019    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      6.041     3.630     8.915     4.974     7.736    0.334     0.656     2.067     17.53     5.285
     Composite CO  :     31.74     30.71     40.55     33.21    125.15     3.014     2.165    12.188    108.23    33.345
     Composite NOX :      0.823     0.912     1.456     1.050     0.864    0.466     0.628     7.763      1.12     1.265
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG  PM-idle  urb  2013QA                                                                                              
* File 1, Run 1, Scenario 15.                                                     
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\IDLE.DEF                                                                  

* Reading Hourly VMT distribution from the following external
* data file: VMT\PMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3426    0.4353    0.1485              0.0193    0.0003    0.0022    0.0497    0.0022    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      6.041     3.630     8.916     4.974     7.649    0.334     0.656     2.034     17.53     5.262
     Composite CO  :     31.74     30.70     40.55     33.21    124.64     3.014     2.165    11.967    108.23    33.504
     Composite NOX :      0.823     0.912     1.456     1.050     0.853    0.466     0.628     7.530      1.12     1.290
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG  PM-idle  sub  2013QA                                                                                              
* File 1, Run 1, Scenario 16.                                                     
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\IDLE.DEF                                                                  

* Reading Hourly VMT distribution from the following external
* data file: VMT\PMPEAK.DEF                                                                  

* Reading Hourly Roadway VMT distribution from the following external
* data file: ..\..\FAC\ART.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.2920    0.4741    0.1618              0.0189    0.0003    0.0024    0.0483    0.0023    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      6.041     3.630     8.918     4.975     7.640    0.334     0.656     2.028     17.53     5.212
     Composite CO  :     31.74     30.71     40.56     33.21    124.62     3.014     2.165    11.913    108.23    33.569
     Composite NOX :      0.823     0.912     1.456     1.051     0.852    0.466     0.628     7.481      1.12     1.290
  ----------------------------------------------------------------------------------------------------------------------
