***************************************************************************
* MOBILE6.2 (31-Oct-2002)                                                 *
* Input file: 01.IN (file 1, run 1).                                      *
***************************************************************************
* Evaluation year 2001 only
* Program data from inspection year 2000
* Basic and Enhanced I/M Programs
* Pass/fail Idle only for all HDGV vehicles >1981
* Colorado 2001 I/M240 cutpoints for cars and trucks

* Reading non-default I/M CUTPOINTS from the following external
* data file: 01CUTPC.D                                                                       

* Reading non-default I/M CUTPOINTS from the following external
* data file: 01CUTPT.D                                                                       
  M616 Comment:
               User has supplied post-1999 sulfur levels.

* Reading Registration Distributions from the following external
* data file: ../../REGDIST/REG_MET.D
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
  M 49 Warning:
                 1.00     MYR sum not = 1. (will normalize)
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   cbd  2001FA                                                                                                      
* File 1, Run 1, Scenario 1.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\CBD.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\CBD.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\CBD.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
*** I/M credits for Tech1&2 vehicles were read from the following external
    data file: TECH12.D                                                                        
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2001
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:  299. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.031
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.5557    0.2769    0.0938              0.0159    0.0013    0.0014    0.0501    0.0050    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      2.260     1.921     4.608     2.601     7.449    1.300     0.995     2.257      9.71     2.503
     Composite CO  :     22.51     24.42     46.68     30.05    113.83     2.818     2.117    13.617     34.10    26.310
     Composite NOX :      1.735     1.489     2.060     1.634     4.371    1.720     1.370    15.248      1.01     2.413
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   frn  2001FA                                                                                                      
* File 1, Run 1, Scenario 2.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\FRN.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\FRN.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\FRN.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2001
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:  299. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.031
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.5128    0.3158    0.1086              0.0168    0.0012    0.0016    0.0402    0.0030    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      2.004     1.723     4.213     2.360     3.104    1.067     0.796     1.425      8.85     2.168
     Composite CO  :     22.87     24.84     46.05     30.26     47.81     2.324     1.703     8.574     29.05    25.812
     Composite NOX :      1.667     1.421     1.970     1.561     4.152    1.672     1.330    16.896      1.17     2.274
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   urb  2001FA                                                                                                      
* File 1, Run 1, Scenario 3.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\URB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\URB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\URB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2001
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:  299. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.031
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4978    0.3218    0.1095              0.0191    0.0012    0.0016    0.0459    0.0030    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      2.007     1.721     4.192     2.348     2.985    1.070     0.800     1.421      8.88     2.164
     Composite CO  :     22.60     24.51     45.57     29.86     45.70     2.333     1.715     8.635     29.26    25.493
     Composite NOX :      1.653     1.404     1.949     1.542     4.091    1.672     1.331    16.218      1.18     2.318
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   sub  2001FA                                                                                                      
* File 1, Run 1, Scenario 4.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\SUB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\SUB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\SUB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2001
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:  299. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.031
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4469    0.3608    0.1234              0.0184    0.0011    0.0018    0.0446    0.0030    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.951     1.680     4.123     2.303     2.731    1.009     0.749     1.271      8.68     2.122
     Composite CO  :     23.11     25.14     46.17     30.50     43.19     2.237     1.634     7.770     28.04    26.325
     Composite NOX :      1.657     1.410     1.957     1.550     4.274    1.729     1.376    16.966      1.23     2.335
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   rur  2001FA                                                                                                      
* File 1, Run 1, Scenario 5.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\RUR.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\RUR.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\RUR.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  

                    Calendar Year:  2001
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:  299. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.031
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.4559    0.3498    0.1194              0.0199    0.0011    0.0018    0.0461    0.0060    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      1.860     1.616     3.941     2.208     2.249    0.927     0.680     1.069      8.73     2.033
     Composite CO  :     24.41     26.71     47.05     31.89     40.62     2.147     1.562     7.057     31.98    27.421
     Composite NOX :      1.694     1.453     1.988     1.589     4.538    2.002     1.599    19.733      1.34     2.531
  ----------------------------------------------------------------------------------------------------------------------
