***************************************************************************
* MOBILE6.2 (31-Oct-2002)                                                 *
* Input file: 13.IN (file 1, run 1).                                      *
***************************************************************************
* Evaluation year 2013 only
* Program data from inspection year 2001
* Basic and Enhanced I/M Programs
* Pass/fail Idle/2500 for all HDGV vehicles >1981
* Colorado 2013 I/M240 cutpoints for cars and trucks

* Reading non-default I/M CUTPOINTS from the following external
* data file: 13CUTPC.D                                                                       

* Reading non-default I/M CUTPOINTS from the following external
* data file: 13CUTPT.D                                                                       
  M616 Comment:
               User has supplied post-1999 sulfur levels.
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   cbd  2013QA                                                                                                      
* File 1, Run 1, Scenario 1.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\CBD.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\CBD.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\CBD.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
*** I/M credits for Tech1&2 vehicles were read from the following external
    data file: TECH12.D                                                                        
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3999    0.3904    0.1331              0.0118    0.0004    0.0019    0.0586    0.0039    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.585     0.684     1.305     0.842     1.786    0.147     0.435     1.081      3.06     0.772
     Composite CO  :     12.61     14.35     18.01     15.28     39.38     1.151     0.934     4.771     27.42    13.896
     Composite NOX :      0.396     0.640     1.128     0.764     1.610    0.215     0.497     6.474      0.88     0.961
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   frn  2013QA                                                                                                      
* File 1, Run 1, Scenario 2.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\FRN.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\FRN.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\FRN.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3584    0.4294    0.1464              0.0168    0.0003    0.0021    0.0447    0.0019    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.504     0.614     1.163     0.753     1.056    0.116     0.345     0.667      2.66     0.668
     Composite CO  :     12.94     14.67     18.36     15.61     25.34     0.908     0.742     2.641     22.96    14.212
     Composite NOX :      0.380     0.613     1.080     0.732     1.378    0.218     0.504     5.082      1.06     0.811
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   urb  2013QA                                                                                                      
* File 1, Run 1, Scenario 3.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\URB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\URB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\URB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3426    0.4353    0.1484              0.0194    0.0003    0.0022    0.0496    0.0022    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.505     0.614     1.162     0.753     1.042    0.116     0.345     0.657      2.68     0.672
     Composite CO  :     12.86     14.59     18.26     15.52     25.15     0.906     0.740     2.581     23.60    14.135
     Composite NOX :      0.378     0.610     1.076     0.729     1.359    0.219     0.504     4.899      1.06     0.828
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   sub  2013QA                                                                                                      
* File 1, Run 1, Scenario 4.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\SUB.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\SUB.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\SUB.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.2920    0.4741    0.1617              0.0190    0.0003    0.0024    0.0482    0.0023    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.491     0.602     1.138     0.739     0.973    0.109     0.325     0.597      2.58     0.667
     Composite CO  :     13.06     14.81     18.52     15.76     23.36     0.860     0.704     2.352     22.01    14.441
     Composite NOX :      0.379     0.612     1.076     0.730     1.397    0.221     0.509     4.933      1.10     0.843
  ----------------------------------------------------------------------------------------------------------------------
 
* # # # # # # # # # # # # # # # # # # # # # # # # #
* DRCOG   rur  2013QA                                                                                                      
* File 1, Run 1, Scenario 5.                                                      
* # # # # # # # # # # # # # # # # # # # # # # # # #

* Reading Hourly, Roadway, and Speed VMT dist. from the following external
* data file: SPEED\RUR.DEF                                                                   

* Reading Hourly VMT distribution from the following external
* data file: VMT\RUR.DEF                                                                     

* Reading Hourly Roadway VMT distribution from the following external
* data file: FACVMT\RUR.DEF

  Reading User Supplied ROADWAY VMT Factors
  M615 Comment:
               User supplied VMT mix.
  M 48 Warning:
              there are no sales for vehicle class HDGV8b  
  M 48 Warning:
              there are no sales for vehicle class LDDT12  

                    Calendar Year:  2013
                            Month:  Jan.
                         Altitude:  High
              Minimum Temperature:  30.0 (F)
              Maximum Temperature:  58.0 (F)
                Absolute Humidity:   75. grains/lb
                 Nominal Fuel RVP:  12.5 psi
                    Weathered RVP:  13.1 psi
              Fuel Sulfur Content:   30. ppm

              Exhaust I/M Program:  Yes 
                 Evap I/M Program:  No  
                      ATP Program:  Yes 
                 Reformulated Gas:  No

   Ether Blend Market Share: 0.000       Alcohol Blend Market Share: 1.000
   Ether Blend Oxygen Content: 0.000     Alcohol Blend Oxygen Content: 0.017
                                          Alcohol Blend RVP Waiver: Yes 

       Vehicle Type:      LDGV    LDGT12    LDGT34      LDGT      HDGV      LDDV      LDDT      HDDV        MC   All Veh
               GVWR:               <6000     >6000     (All)
                        ------    ------    ------    ------    ------    ------    ------    ------    ------    ------
   VMT Distribution:    0.3010    0.4631    0.1579              0.0203    0.0003    0.0023    0.0502    0.0049    1.0000
  ----------------------------------------------------------------------------------------------------------------------
 Composite Emission Factors (g/mi):
     Composite VOC :      0.475     0.589     1.106     0.721     0.895    0.102     0.305     0.531      2.65     0.649
     Composite CO  :     13.56     15.37     19.20     16.34     23.63     0.841     0.689     2.221     25.78    14.953
     Composite NOX :      0.389     0.623     1.089     0.741     1.453    0.251     0.579     5.524      1.18     0.891
  ----------------------------------------------------------------------------------------------------------------------
***************************************************************************
* MOBILE6.2 (31-Oct-2002)                                                 *
* Input file: 13.IN (file 1, run 2).                                      *
***************************************************************************
